**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No: 41-G001-25**

## Specification

### Background

The fencing of the Processing Center/Office building is part of the upgrading at CPPL Kiritimati Branch. This upgrade is essential in order to align with the Competent Authority (CA) requirements, as Kiritimati Branch will be involved in export.

These regulations mandate that processing facilities of Seafood maintain a controlled and secure environment, including measures to prevent animal intrusion and ensure compliance with hygiene and safety standards. The absence of a proper fence poses risks such as contamination from stray animals and unauthorized access, which could jeopardize product quality and export eligibility.

**The objectives of the project include:**

* To prevent animal intrusion wherein keeping pests away from the fish processing areas and minimize the risk of cross contamination and ensures a hygienic environment for production
* To establish a defined perimeter which will help regulate access to the processing and office areas, improving operation security.
* To meet export standards specifically the CA regulations for maintaining and expanding export opportunities.

To meet the Project’s objective, Government is seeking submission of tenders for the following specification and requirements:

### Requirements

### Please refer to RFQ Instruction on how to submit the Quotation part II - “Quotation Documents Required to be Submitted”.

### Including the following certificate- Certified & valid Business registration certificate, Valid operational business license, and tax clearance document, specification of the product and recent photos (not exceeds 1 month) and nature of business

### Installation services

Technical assistance for the installation and servicing services may not be necessary in the supply of Fence Materials.

### Delivery Time

The fence materials shall be delivered not more than 2 months from the date of receiving the payment.

## Description of the Goods

The tenderers are required to provide a quotation for CPPL Processing Center/Office Building Fence according to specification requirements appended below.

The specifications of the **Fence Materials** are appended below:

|  |  |  |
| --- | --- | --- |
| **Description** | **Qty** | **Unit** |
| Concrete block 400 x200 x 150 | 2165 | nos |
| Portland Cement 40kg - footing | 84 | bags |
| Portland Cement 40kg – Mortar/grouting | 90 | bags |
| Rod deformed 12mmØ x 6m - footing | 76 | lengths |
| Rod deformed 12mmØ x 6m - starter bar | 31 | lengths |
| Rod plain 6mmØ x 6m | 24 | lengths |
| Tie wire 120m roll | 4 | kg/rolls |
| C-Grade galv pipe 50mm | 26 | lengths |
| Galv chainlink fence 50mm x 15m | 9 | rolls |
| Gallvanised wire wire #8G (4mm) 230m | 2 | rolls |
| Barbed wire 18kg x 360m | 2 |  |