**REQUEST FOR QUOTATION  
SPECIFICATION OF STANDARD GOODS**

**Procurement No:** **46-G010-24**

## Specification

### Background

The project is aimed to boost the Branch sales and to comply with safety reasons

### Requirements

All supporting documentation must be in English.

### Installation services

Not applicable

### Delivery Time

One Month

## Description of the Goods

*Here, list all items to be Tendered*

*(This part may be replaced by a proprietary Supplier description)*

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Pos. | Description | Number | Delivery Time (to be Tendered) | Price (to be Tendered) |
| 1 | ENGRO HIGH GRADE PORTLAND CEMENT 50KGS BAG STRENGTH CLASS 42.5 IS USED IN CONCRETE, PRECAST AND MASONARY PRODUCTS FOR A MULTIITUDE OF CONSTRUCTION PROJECTS INCLUDING HIGH RISE OFFICE BUILDINGS ROAD WAY BRIDGES AND PAVEMENTS AND RESIDENTIAL FOUNDATION AND DRIVE WAYS. | 800 bags | 1 mont |  |
| 2 |  |  |  |  |
| 3 |  |  |  |  |
| 4 |  |  |  |  |